WILT Procedure:

1. Start Dryer (Tech needs to start) – Waiting for Dryer Start
2. Dry for 2 min – Drying Clothes
3. Inject Water for 2 minutes – Water Injection 1
4. Pause Station – Pause Dryer
5. Start Station – Sending Manual Start Stop Command
6. Dry for 2 min – Drying Clothes
7. Inject Water for 2 min – Water Injection 2
8. Dry Cloths – Drying Clothes
9. Cool Down Period – Cooling Down
10. Restart Dryer - Sending Manual Start Stop Command

Enum Test State Commands:

No Serial Number

Waiting for Dryer Start

Drying Clothes

Water Injection 1

Pause Dryer

Sending Manual Start Stop Command

Water Injection 2

Cooling Down

Fault